To verify the serial connectivity and configure static route

















